(export (version D)
  (design
    (source /home/user/workspace/NoPCShare/IotTeam/VinhomeDoor/Sources/Hardware/vinhome/vinhome.sch)
    (date "Tue 25 Sep 2018 10:27:06 AM +07")
    (tool "Eeschema (5.0.0-rc2-109-g0e3be5776-dirty)-sonnt")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source vinhome.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 2) (name /Sheet5B616227/) (tstamps /5B616228/)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source display.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 3) (name /Sheet5B6162EB/) (tstamps /5B6162EC/)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source motor.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 4) (name /Sheet5B6C14E0/) (tstamps /5B6C14E1/)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source main.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 5) (name /Sheet5B6C3003/) (tstamps /5B6C3004/)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source atmega328.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 6) (name /Sheet5B71ECCF/) (tstamps /5B71ECD0/)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source RFID.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 7) (name /ADC/) (tstamps /5B9F7E36/)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source file5B9F7E35.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 8) (name /Sheet5B629A41/) (tstamps /5B629A42/)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source keypad.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 9) (name /Sheet5B71E55C/) (tstamps /5B71E55D/)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source connectorsch.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref R9)
      (value 100R)
      (footprint Resistors_SMD:R_0805_HandSoldering)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /Sheet5B616227/) (tstamps /5B616228/))
      (tstamp 5B73F886))
    (comp (ref Q2)
      (value BC807)
      (footprint TO_SOT_Packages_SMD:SOT-23)
      (datasheet http://www.fairchildsemi.com/ds/BC/BC807.pdf)
      (libsource (lib Transistor) (part BC807) (description "0.8A Ic, 45V Vce, PNP Transistor, SOT-23"))
      (sheetpath (names /Sheet5B616227/) (tstamps /5B616228/))
      (tstamp 5B740909))
    (comp (ref C15)
      (value 104)
      (footprint Capacitors_SMD:C_0805)
      (libsource (lib device) (part C_Small) (description "Unpolarized capacitor"))
      (sheetpath (names /Sheet5B616227/) (tstamps /5B616228/))
      (tstamp 5B765EF1))
    (comp (ref J1)
      (value lcd)
      (footprint Pin_Headers:Pin_Header_Straight_1x09_Pitch2.54mm)
      (datasheet ~)
      (libsource (lib Connector) (part Conn_01x09) (description "Generic connector, single row, 01x09"))
      (sheetpath (names /Sheet5B616227/) (tstamps /5B616228/))
      (tstamp 5B7AC080))
    (comp (ref J7)
      (value SD_card)
      (footprint Pin_Headers:Pin_Header_Straight_1x06_Pitch2.54mm)
      (datasheet ~)
      (libsource (lib Connector) (part Conn_01x06) (description "Generic connector, single row, 01x06"))
      (sheetpath (names /Sheet5B616227/) (tstamps /5B616228/))
      (tstamp 5B7AD180))
    (comp (ref C16)
      (value 104)
      (footprint Capacitors_SMD:C_0805)
      (libsource (lib device) (part C_Small) (description "Unpolarized capacitor"))
      (sheetpath (names /Sheet5B616227/) (tstamps /5B616228/))
      (tstamp 5B7AD6EA))
    (comp (ref J2)
      (value "power 12V")
      (footprint Connectors_Terminal_Blocks:TerminalBlock_Philmore_TB132_02x5mm_Straight)
      (datasheet ~)
      (libsource (lib Connector) (part Conn_01x02) (description "Generic connector, single row, 01x02"))
      (sheetpath (names /Sheet5B6162EB/) (tstamps /5B6162EC/))
      (tstamp 5B62FA88))
    (comp (ref R1)
      (value 10R)
      (footprint Resistors_SMD:R_0805)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /Sheet5B6162EB/) (tstamps /5B6162EC/))
      (tstamp 5B63085B))
    (comp (ref D1)
      (value D_Schottky)
      (footprint Diodes_SMD:D_SMB_Handsoldering)
      (libsource (lib device) (part D_Schottky) (description "Schottky diode"))
      (sheetpath (names /Sheet5B6162EB/) (tstamps /5B6162EC/))
      (tstamp 5B631428))
    (comp (ref R2)
      (value 47k)
      (footprint Resistors_SMD:R_0805)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /Sheet5B6162EB/) (tstamps /5B6162EC/))
      (tstamp 5B632236))
    (comp (ref Q1)
      (value Q_NMOS_GSD)
      (footprint TO_SOT_Packages_SMD:SOT-23)
      (libsource (lib device) (part Q_NMOS_GSD) (description "Transistor N-MOSFETwith substrate diode (general)"))
      (sheetpath (names /Sheet5B6162EB/) (tstamps /5B6162EC/))
      (tstamp 5B633A97))
    (comp (ref C2)
      (value 104)
      (footprint Capacitors_SMD:C_0805_HandSoldering)
      (libsource (lib device) (part C_Small) (description "Unpolarized capacitor"))
      (sheetpath (names /Sheet5B6162EB/) (tstamps /5B6162EC/))
      (tstamp 5B63429C))
    (comp (ref C4)
      (value 104)
      (footprint Capacitors_SMD:C_0805_HandSoldering)
      (libsource (lib device) (part C_Small) (description "Unpolarized capacitor"))
      (sheetpath (names /Sheet5B6162EB/) (tstamps /5B6162EC/))
      (tstamp 5B6349A5))
    (comp (ref U1)
      (value HX_mini_360)
      (footprint iot:hx_mini_360)
      (libsource (lib vinhome-rescue) (part HX_mini_360-lanhnd) (description ""))
      (sheetpath (names /Sheet5B6162EB/) (tstamps /5B6162EC/))
      (tstamp 5B67BC79))
    (comp (ref J3)
      (value conn_chotcua)
      (footprint Pin_Headers:Pin_Header_Straight_1x06_Pitch2.54mm)
      (datasheet ~)
      (libsource (lib Connector) (part Conn_01x06) (description "Generic connector, single row, 01x06"))
      (sheetpath (names /Sheet5B6162EB/) (tstamps /5B6162EC/))
      (tstamp 5BA253C5))
    (comp (ref C1)
      (value 106)
      (footprint Capacitors_SMD:C_0805_HandSoldering)
      (libsource (lib device) (part C_Small) (description "Unpolarized capacitor"))
      (sheetpath (names /Sheet5B6162EB/) (tstamps /5B6162EC/))
      (tstamp 5BA5461E))
    (comp (ref C3)
      (value 106)
      (footprint Capacitors_SMD:C_0805_HandSoldering)
      (libsource (lib device) (part C_Small) (description "Unpolarized capacitor"))
      (sheetpath (names /Sheet5B6162EB/) (tstamps /5B6162EC/))
      (tstamp 5BA54720))
    (comp (ref U2)
      (value ESP-12E)
      (footprint ESP8266:ESP-12E_SMD)
      (libsource (lib ESP8266) (part ESP-12E) (description ""))
      (sheetpath (names /Sheet5B6C14E0/) (tstamps /5B6C14E1/))
      (tstamp 5B61664F))
    (comp (ref C8)
      (value 105)
      (footprint Capacitors_SMD:C_0805_HandSoldering)
      (libsource (lib device) (part C_Small) (description "Unpolarized capacitor"))
      (sheetpath (names /Sheet5B6C14E0/) (tstamps /5B6C14E1/))
      (tstamp 5B618730))
    (comp (ref R3)
      (value 12k)
      (footprint Resistors_SMD:R_0805_HandSoldering)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /Sheet5B6C14E0/) (tstamps /5B6C14E1/))
      (tstamp 5B61A13D))
    (comp (ref R4)
      (value 12k)
      (footprint Resistors_SMD:R_0805_HandSoldering)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /Sheet5B6C14E0/) (tstamps /5B6C14E1/))
      (tstamp 5B61A490))
    (comp (ref R5)
      (value 12k)
      (footprint Resistors_SMD:R_0805_HandSoldering)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /Sheet5B6C14E0/) (tstamps /5B6C14E1/))
      (tstamp 5B61A4C8))
    (comp (ref R6)
      (value 12k)
      (footprint Resistors_SMD:R_0805_HandSoldering)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /Sheet5B6C14E0/) (tstamps /5B6C14E1/))
      (tstamp 5B61A4EA))
    (comp (ref R7)
      (value 12k)
      (footprint Resistors_SMD:R_0805_HandSoldering)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /Sheet5B6C14E0/) (tstamps /5B6C14E1/))
      (tstamp 5B61A5B4))
    (comp (ref C7)
      (value 103)
      (footprint Capacitors_SMD:C_0805)
      (libsource (lib device) (part C_Small) (description "Unpolarized capacitor"))
      (sheetpath (names /Sheet5B6C14E0/) (tstamps /5B6C14E1/))
      (tstamp 5B620CF1))
    (comp (ref C6)
      (value 104)
      (footprint Capacitors_SMD:C_0805)
      (libsource (lib device) (part C_Small) (description "Unpolarized capacitor"))
      (sheetpath (names /Sheet5B6C14E0/) (tstamps /5B6C14E1/))
      (tstamp 5B6C7440))
    (comp (ref R11)
      (value 12k)
      (footprint Resistors_SMD:R_0805)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /Sheet5B6C14E0/) (tstamps /5B6C14E1/))
      (tstamp 5B748144))
    (comp (ref R10)
      (value 12k)
      (footprint Resistors_SMD:R_0805)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /Sheet5B6C14E0/) (tstamps /5B6C14E1/))
      (tstamp 5B7483AD))
    (comp (ref Q3)
      (value MMBT9018)
      (footprint TO_SOT_Packages_SMD:SOT-23)
      (datasheet http://www.onsemi.com/pub_link/Collateral/2N2219-D.PDF)
      (libsource (lib Transistor) (part 2N2219) (description "800mA Ic, 50V Vce, NPN Transistor, TO-39"))
      (sheetpath (names /Sheet5B6C14E0/) (tstamps /5B6C14E1/))
      (tstamp 5B748949))
    (comp (ref Q4)
      (value MMBT9018)
      (footprint TO_SOT_Packages_SMD:SOT-23)
      (datasheet http://www.onsemi.com/pub_link/Collateral/2N2219-D.PDF)
      (libsource (lib Transistor) (part 2N2219) (description "800mA Ic, 50V Vce, NPN Transistor, TO-39"))
      (sheetpath (names /Sheet5B6C14E0/) (tstamps /5B6C14E1/))
      (tstamp 5B7499E4))
    (comp (ref J5)
      (value Conn_01x06)
      (footprint Pin_Headers:Pin_Header_Straight_1x06_Pitch2.54mm)
      (datasheet ~)
      (libsource (lib Connector) (part Conn_01x06) (description "Generic connector, single row, 01x06"))
      (sheetpath (names /Sheet5B6C14E0/) (tstamps /5B6C14E1/))
      (tstamp 5B755821))
    (comp (ref R12)
      (value 220R)
      (footprint Resistors_SMD:R_0805)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /Sheet5B6C14E0/) (tstamps /5B6C14E1/))
      (tstamp 5B77A49F))
    (comp (ref U3)
      (value ATMEGA328P-AU)
      (footprint Housings_QFP:TQFP-32_7x7mm_Pitch0.8mm)
      (datasheet http://www.atmel.com/images/atmel-8271-8-bit-avr-microcontroller-atmega48a-48pa-88a-88pa-168a-168pa-328-328p_datasheet.pdf)
      (libsource (lib atmel) (part ATMEGA328P-AU) (description "TQFP32, 32k Flash, 2kB SRAM, 1kB EEPROM"))
      (sheetpath (names /Sheet5B6C3003/) (tstamps /5B6C3004/))
      (tstamp 5B6CC01A))
    (comp (ref C10)
      (value 104)
      (footprint Capacitors_SMD:C_0805_HandSoldering)
      (libsource (lib device) (part C_Small) (description "Unpolarized capacitor"))
      (sheetpath (names /Sheet5B6C3003/) (tstamps /5B6C3004/))
      (tstamp 5B6CC796))
    (comp (ref C11)
      (value 20pF)
      (footprint Capacitors_SMD:C_0805_HandSoldering)
      (libsource (lib device) (part C_Small) (description "Unpolarized capacitor"))
      (sheetpath (names /Sheet5B6C3003/) (tstamps /5B6C3004/))
      (tstamp 5B6CD364))
    (comp (ref C12)
      (value 20pF)
      (footprint Capacitors_SMD:C_0805_HandSoldering)
      (libsource (lib device) (part C_Small) (description "Unpolarized capacitor"))
      (sheetpath (names /Sheet5B6C3003/) (tstamps /5B6C3004/))
      (tstamp 5B6CD756))
    (comp (ref C9)
      (value 104)
      (footprint Capacitors_SMD:C_0805)
      (libsource (lib device) (part C_Small) (description "Unpolarized capacitor"))
      (sheetpath (names /Sheet5B6C3003/) (tstamps /5B6C3004/))
      (tstamp 5B6DC171))
    (comp (ref R8)
      (value 10k)
      (footprint Resistors_SMD:R_0805_HandSoldering)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /Sheet5B6C3003/) (tstamps /5B6C3004/))
      (tstamp 5B6EB8E6))
    (comp (ref J6)
      (value Conn_01x08)
      (footprint Pin_Headers:Pin_Header_Straight_1x08_Pitch2.54mm)
      (datasheet ~)
      (libsource (lib Connector) (part Conn_01x08) (description "Generic connector, single row, 01x08"))
      (sheetpath (names /Sheet5B6C3003/) (tstamps /5B6C3004/))
      (tstamp 5B7787F8))
    (comp (ref R14)
      (value 10k)
      (footprint Resistors_SMD:R_0805)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /Sheet5B6C3003/) (tstamps /5B6C3004/))
      (tstamp 5B77D8B7))
    (comp (ref R13)
      (value 10k)
      (footprint Resistors_SMD:R_0805)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /Sheet5B6C3003/) (tstamps /5B6C3004/))
      (tstamp 5B77D98E))
    (comp (ref Y1)
      (value Crystal_GND24)
      (footprint Crystals:Crystal_SMD_3225-4pin_3.2x2.5mm)
      (libsource (lib device) (part Crystal_GND24) (description "Four pin crystal (GND on pins 2 and 4), e.g. in SMD package"))
      (sheetpath (names /Sheet5B6C3003/) (tstamps /5B6C3004/))
      (tstamp 5BA8A92C))
    (comp (ref J11)
      (value RFID_RC522)
      (footprint Pin_Headers:Pin_Header_Straight_1x08_Pitch2.54mm)
      (datasheet ~)
      (libsource (lib Connector) (part Conn_01x08) (description "Generic connector, single row, 01x08"))
      (sheetpath (names /Sheet5B71ECCF/) (tstamps /5B71ECD0/))
      (tstamp 5B71F223))
    (comp (ref C14)
      (value 104)
      (footprint Capacitors_SMD:C_0805)
      (libsource (lib device) (part C_Small) (description "Unpolarized capacitor"))
      (sheetpath (names /Sheet5B71ECCF/) (tstamps /5B71ECD0/))
      (tstamp 5B76BCD3))
    (comp (ref MK1)
      (value Microphone)
      (footprint Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm)
      (libsource (lib device) (part Microphone) (description Microphone))
      (sheetpath (names /ADC/) (tstamps /5B9F7E36/))
      (tstamp 5B9F91FA))
    (comp (ref R15)
      (value 82k)
      (footprint Resistors_SMD:R_0805_HandSoldering)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /ADC/) (tstamps /5B9F7E36/))
      (tstamp 5BA0C54D))
    (comp (ref C5)
      (value 1uF)
      (footprint Capacitors_SMD:C_0805_HandSoldering)
      (libsource (lib device) (part CP_Small) (description "Polarised capacitor"))
      (sheetpath (names /ADC/) (tstamps /5B9F7E36/))
      (tstamp 5BA0C6FA))
    (comp (ref R16)
      (value 200k)
      (footprint Resistors_SMD:R_0805_HandSoldering)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /ADC/) (tstamps /5B9F7E36/))
      (tstamp 5BA1DBD8))
    (comp (ref Q5)
      (value TRANSISTOR_NPNSOT23-3)
      (footprint TO_SOT_Packages_SMD:SOT-23W)
      (libsource (lib vinhome-rescue) (part TRANSISTOR_NPNSOT23-3-SparkFun-DiscreteSemi) (description ""))
      (sheetpath (names /ADC/) (tstamps /5B9F7E36/))
      (tstamp 5BA1DE3C))
    (comp (ref R18)
      (value 10k)
      (footprint Resistors_SMD:R_0805_HandSoldering)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /ADC/) (tstamps /5B9F7E36/))
      (tstamp 5BA1E5F9))
    (comp (ref C17)
      (value 10UF)
      (footprint Capacitors_SMD:C_0805_HandSoldering)
      (libsource (lib device) (part CP_Small) (description "Polarised capacitor"))
      (sheetpath (names /ADC/) (tstamps /5B9F7E36/))
      (tstamp 5BA1F841))
    (comp (ref R19)
      (value 100R)
      (footprint Resistors_SMD:R_0805_HandSoldering)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /ADC/) (tstamps /5B9F7E36/))
      (tstamp 5BA1E674))
    (comp (ref J4)
      (value camera)
      (footprint Pin_Headers:Pin_Header_Straight_1x05_Pitch2.54mm)
      (datasheet ~)
      (libsource (lib Connector) (part Conn_01x05) (description "Generic connector, single row, 01x05"))
      (sheetpath (names /Sheet5B629A41/) (tstamps /5B629A42/))
      (tstamp 5B9F95E5))
    (comp (ref U4)
      (value Pam_8403_audio)
      (footprint iot:PAM8403_module)
      (libsource (lib lanhnd) (part Pam_8403_audio) (description ""))
      (sheetpath (names /Sheet5B629A41/) (tstamps /5B629A42/))
      (tstamp 5BA39C8E))
    (comp (ref J10)
      (value Conn_01x02)
      (footprint Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm)
      (datasheet ~)
      (libsource (lib Connector) (part Conn_01x02) (description "Generic connector, single row, 01x02"))
      (sheetpath (names /Sheet5B629A41/) (tstamps /5B629A42/))
      (tstamp 5BA39908))
    (comp (ref J9)
      (value Conn_01x02)
      (footprint Pin_Headers:Pin_Header_Straight_1x02_Pitch2.54mm)
      (datasheet ~)
      (libsource (lib Connector) (part Conn_01x02) (description "Generic connector, single row, 01x02"))
      (sheetpath (names /Sheet5B629A41/) (tstamps /5B629A42/))
      (tstamp 5BA3A1A4))
    (comp (ref C13)
      (value 104)
      (footprint Capacitors_SMD:C_0805)
      (libsource (lib device) (part C_Small) (description "Unpolarized capacitor"))
      (sheetpath (names /Sheet5B71E55C/) (tstamps /5B71E55D/))
      (tstamp 5B6EF154))
    (comp (ref J8)
      (value keypad)
      (footprint Pin_Headers:Pin_Header_Straight_1x06_Pitch2.54mm)
      (datasheet ~)
      (libsource (lib Connector) (part Conn_01x06) (description "Generic connector, single row, 01x06"))
      (sheetpath (names /Sheet5B71E55C/) (tstamps /5B71E55D/))
      (tstamp 5BA007CB)))
  (libparts
    (libpart (lib Connector) (part Conn_01x02)
      (description "Generic connector, single row, 01x02")
      (docs ~)
      (footprints
        (fp Connector*:*_??x*mm*)
        (fp Connector*:*1x??x*mm*)
        (fp Pin?Header?Straight?1X*)
        (fp Pin?Header?Angled?1X*)
        (fp Socket?Strip?Straight?1X*)
        (fp Socket?Strip?Angled?1X*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x02))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))))
    (libpart (lib Connector) (part Conn_01x05)
      (description "Generic connector, single row, 01x05")
      (docs ~)
      (footprints
        (fp Connector*:*_??x*mm*)
        (fp Connector*:*1x??x*mm*)
        (fp Pin?Header?Straight?1X*)
        (fp Pin?Header?Angled?1X*)
        (fp Socket?Strip?Straight?1X*)
        (fp Socket?Strip?Angled?1X*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x05))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))
        (pin (num 4) (name Pin_4) (type passive))
        (pin (num 5) (name Pin_5) (type passive))))
    (libpart (lib Connector) (part Conn_01x06)
      (description "Generic connector, single row, 01x06")
      (docs ~)
      (footprints
        (fp Connector*:*_??x*mm*)
        (fp Connector*:*1x??x*mm*)
        (fp Pin?Header?Straight?1X*)
        (fp Pin?Header?Angled?1X*)
        (fp Socket?Strip?Straight?1X*)
        (fp Socket?Strip?Angled?1X*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x06))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))
        (pin (num 4) (name Pin_4) (type passive))
        (pin (num 5) (name Pin_5) (type passive))
        (pin (num 6) (name Pin_6) (type passive))))
    (libpart (lib Connector) (part Conn_01x08)
      (description "Generic connector, single row, 01x08")
      (docs ~)
      (footprints
        (fp Connector*:*_??x*mm*)
        (fp Connector*:*1x??x*mm*)
        (fp Pin?Header?Straight?1X*)
        (fp Pin?Header?Angled?1X*)
        (fp Socket?Strip?Straight?1X*)
        (fp Socket?Strip?Angled?1X*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x08))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))
        (pin (num 4) (name Pin_4) (type passive))
        (pin (num 5) (name Pin_5) (type passive))
        (pin (num 6) (name Pin_6) (type passive))
        (pin (num 7) (name Pin_7) (type passive))
        (pin (num 8) (name Pin_8) (type passive))))
    (libpart (lib Connector) (part Conn_01x09)
      (description "Generic connector, single row, 01x09")
      (docs ~)
      (footprints
        (fp Connector*:*_??x*mm*)
        (fp Connector*:*1x??x*mm*)
        (fp Pin?Header?Straight?1X*)
        (fp Pin?Header?Angled?1X*)
        (fp Socket?Strip?Straight?1X*)
        (fp Socket?Strip?Angled?1X*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x09))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))
        (pin (num 4) (name Pin_4) (type passive))
        (pin (num 5) (name Pin_5) (type passive))
        (pin (num 6) (name Pin_6) (type passive))
        (pin (num 7) (name Pin_7) (type passive))
        (pin (num 8) (name Pin_8) (type passive))
        (pin (num 9) (name Pin_9) (type passive))))
    (libpart (lib ESP8266) (part ESP-12E)
      (footprints
        (fp ESP-12E)
        (fp ESP-12E_SMD))
      (fields
        (field (name Reference) U)
        (field (name Value) ESP-12E))
      (pins
        (pin (num 1) (name REST) (type input))
        (pin (num 2) (name ADC) (type passive))
        (pin (num 3) (name CH_PD) (type input))
        (pin (num 4) (name GPIO16) (type BiDi))
        (pin (num 5) (name GPIO14) (type BiDi))
        (pin (num 6) (name GPIO12) (type BiDi))
        (pin (num 7) (name GPIO13) (type BiDi))
        (pin (num 8) (name VCC) (type power_in))
        (pin (num 9) (name GND) (type power_in))
        (pin (num 10) (name GPIO15) (type BiDi))
        (pin (num 11) (name GPIO2) (type BiDi))
        (pin (num 12) (name GPIO0) (type BiDi))
        (pin (num 13) (name GPIO4) (type BiDi))
        (pin (num 14) (name GPIO5) (type BiDi))
        (pin (num 15) (name RXD) (type input))
        (pin (num 16) (name TXD) (type output))
        (pin (num 17) (name CS0) (type BiDi))
        (pin (num 18) (name MISO) (type BiDi))
        (pin (num 19) (name GPIO9) (type BiDi))
        (pin (num 20) (name GPIO10) (type BiDi))
        (pin (num 21) (name MOSI) (type BiDi))
        (pin (num 22) (name SCLK) (type BiDi))))
    (libpart (lib Transistor) (part 2N2219)
      (aliases
        (alias BC140)
        (alias BC141))
      (description "800mA Ic, 50V Vce, NPN Transistor, TO-39")
      (docs http://www.onsemi.com/pub_link/Collateral/2N2219-D.PDF)
      (footprints
        (fp TO?39*))
      (fields
        (field (name Reference) Q)
        (field (name Value) 2N2219)
        (field (name Footprint) TO_SOT_Packages_THT:TO-39-3))
      (pins
        (pin (num 1) (name E) (type passive))
        (pin (num 2) (name B) (type passive))
        (pin (num 3) (name C) (type passive))))
    (libpart (lib Transistor) (part BC807)
      (aliases
        (alias BC808)
        (alias BC856)
        (alias BC857)
        (alias BC858)
        (alias BC859)
        (alias BC860)
        (alias MMBT3906))
      (description "0.8A Ic, 45V Vce, PNP Transistor, SOT-23")
      (docs http://www.fairchildsemi.com/ds/BC/BC807.pdf)
      (footprints
        (fp SOT?23*))
      (fields
        (field (name Reference) Q)
        (field (name Value) BC807)
        (field (name Footprint) TO_SOT_Packages_SMD:SOT-23))
      (pins
        (pin (num 1) (name B) (type input))
        (pin (num 2) (name E) (type passive))
        (pin (num 3) (name C) (type passive))))
    (libpart (lib atmel) (part ATMEGA168A-AU)
      (aliases
        (alias ATMEGA48A-AU)
        (alias ATMEGA48PA-AU)
        (alias ATMEGA88A-AU)
        (alias ATMEGA88PA-AU)
        (alias ATMEGA168PA-AU)
        (alias ATMEGA328-AU)
        (alias ATMEGA328P-AU))
      (description "TQFP32, 16k Flash, 1kB SRAM, 512B EEPROM")
      (docs http://www.atmel.com/images/atmel-8271-8-bit-avr-microcontroller-atmega48a-48pa-88a-88pa-168a-168pa-328-328p_datasheet.pdf)
      (footprints
        (fp TQFP*7x7mm*Pitch0.8mm*))
      (fields
        (field (name Reference) U)
        (field (name Value) ATMEGA168A-AU)
        (field (name Footprint) Housings_QFP:TQFP-32_7x7mm_Pitch0.8mm))
      (pins
        (pin (num 1) (name "(PCINT19/OC2B/INT1)PD3") (type BiDi))
        (pin (num 2) (name "(PCINT20/XCK/T0)PD4") (type BiDi))
        (pin (num 3) (name GND) (type power_in))
        (pin (num 4) (name VCC) (type power_in))
        (pin (num 5) (name GND) (type power_in))
        (pin (num 6) (name VCC) (type power_in))
        (pin (num 7) (name "(PCINT6/XTAL1/TOSC1)PB6") (type BiDi))
        (pin (num 8) (name "(PCINT7/XTAL2/TOSC2)PB7") (type BiDi))
        (pin (num 9) (name "(PCINT21/OC0B/T1)PD5") (type BiDi))
        (pin (num 10) (name "(PCINT22/OC0A/AIN0)PD6") (type BiDi))
        (pin (num 11) (name "(PCINT23/AIN1)PD7") (type BiDi))
        (pin (num 12) (name "(PCINT0/CLKO/ICP1)PB0") (type BiDi))
        (pin (num 13) (name "(PCINT1/OC1A)PB1") (type BiDi))
        (pin (num 14) (name "(PCINT2/OC1B/~SS~)PB2") (type BiDi))
        (pin (num 15) (name "(PCINT3/OC2A/MOSI)PB3") (type BiDi))
        (pin (num 16) (name "(PCINT4/MISO)PB4") (type BiDi))
        (pin (num 17) (name "(PCINT5/SCK)PB5") (type BiDi))
        (pin (num 18) (name AVCC) (type power_in))
        (pin (num 19) (name ADC6) (type input))
        (pin (num 20) (name AREF) (type BiDi))
        (pin (num 21) (name GND) (type power_in))
        (pin (num 22) (name ADC7) (type input))
        (pin (num 23) (name "(PCINT8/ADC0)PC0") (type BiDi))
        (pin (num 24) (name "(PCINT9/ADC1)PC1") (type BiDi))
        (pin (num 25) (name "(PCINT10/ADC2)PC2") (type BiDi))
        (pin (num 26) (name "(PCINT11/ADC3)PC3") (type BiDi))
        (pin (num 27) (name "(PCINT12/SDA/ADC4)PC4") (type BiDi))
        (pin (num 28) (name "(PCINT13/SCL/ADC5)PC5") (type BiDi))
        (pin (num 29) (name "(PCINT14/~RESET~)PC6") (type BiDi))
        (pin (num 30) (name "(PCINT16/RXD)PD0") (type BiDi))
        (pin (num 31) (name "(PCINT17/TXD)PD1") (type BiDi))
        (pin (num 32) (name "(PCINT18/INT0)PD2") (type BiDi))))
    (libpart (lib device) (part CP_Small)
      (description "Polarised capacitor")
      (footprints
        (fp CP_*))
      (fields
        (field (name Reference) C)
        (field (name Value) CP_Small))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib device) (part C_Small)
      (description "Unpolarized capacitor")
      (footprints
        (fp C_*))
      (fields
        (field (name Reference) C)
        (field (name Value) C_Small))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib device) (part Crystal_GND24)
      (description "Four pin crystal (GND on pins 2 and 4), e.g. in SMD package")
      (footprints
        (fp Crystal*))
      (fields
        (field (name Reference) Y)
        (field (name Value) Crystal_GND24))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))
        (pin (num 3) (name 3) (type passive))
        (pin (num 4) (name 4) (type passive))))
    (libpart (lib device) (part D_Schottky)
      (description "Schottky diode")
      (footprints
        (fp TO-???*)
        (fp *SingleDiode)
        (fp *_Diode_*)
        (fp *SingleDiode*)
        (fp D_*))
      (fields
        (field (name Reference) D)
        (field (name Value) D_Schottky))
      (pins
        (pin (num 1) (name K) (type passive))
        (pin (num 2) (name A) (type passive))))
    (libpart (lib device) (part Microphone)
      (description Microphone)
      (fields
        (field (name Reference) MK)
        (field (name Value) Microphone))
      (pins
        (pin (num 1) (name -) (type passive))
        (pin (num 2) (name +) (type passive))))
    (libpart (lib device) (part Q_NMOS_GSD)
      (description "Transistor N-MOSFETwith substrate diode (general)")
      (fields
        (field (name Reference) Q)
        (field (name Value) Q_NMOS_GSD))
      (pins
        (pin (num 1) (name G) (type input))
        (pin (num 2) (name S) (type passive))
        (pin (num 3) (name D) (type passive))))
    (libpart (lib device) (part R)
      (description Resistor)
      (footprints
        (fp R_*)
        (fp R_*))
      (fields
        (field (name Reference) R)
        (field (name Value) R))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib lanhnd) (part Pam_8403_audio)
      (fields
        (field (name Reference) U)
        (field (name Value) Pam_8403_audio))
      (pins
        (pin (num 1) (name GND) (type input))
        (pin (num 2) (name VCC) (type input))
        (pin (num 3) (name L_IN) (type input))
        (pin (num 4) (name GND) (type input))
        (pin (num 5) (name R_IN) (type input))
        (pin (num 6) (name OUT_L-) (type input))
        (pin (num 7) (name OUT_L+) (type input))
        (pin (num 8) (name OUT_R-) (type input))
        (pin (num 9) (name OUT_R+) (type input))))
    (libpart (lib vinhome-rescue) (part HX_mini_360-lanhnd)
      (fields
        (field (name Reference) U)
        (field (name Value) HX_mini_360-lanhnd))
      (pins
        (pin (num 1) (name IN+) (type input))
        (pin (num 2) (name OUT+) (type input))
        (pin (num 3) (name OUT-) (type input))
        (pin (num 4) (name IN-) (type input))))
    (libpart (lib vinhome-rescue) (part TRANSISTOR_NPNSOT23-3-SparkFun-DiscreteSemi)
      (footprints
        (fp *SOT23-3*))
      (fields
        (field (name Reference) Q)
        (field (name Value) TRANSISTOR_NPNSOT23-3-SparkFun-DiscreteSemi)
        (field (name Footprint) SOT23-3))
      (pins
        (pin (num 1) (name B) (type passive))
        (pin (num 2) (name E) (type passive))
        (pin (num 3) (name C) (type passive)))))
  (libraries
    (library (logical Connector)
      (uri /usr/share/kicad/library//Connector.lib))
    (library (logical ESP8266)
      (uri /home/user/userlibs/kicad-library/userlibs//ESP8266.lib))
    (library (logical Transistor)
      (uri /usr/share/kicad/library//Transistor.lib))
    (library (logical atmel)
      (uri /usr/share/kicad/library//atmel.lib))
    (library (logical device)
      (uri /usr/share/kicad/library//device.lib))
    (library (logical lanhnd)
      (uri /home/user/workspace/NoPCShare/public/DataPublic/sonnt/libraries/kicad-library/userlibs//lanhnd/lanhnd.lib))
    (library (logical vinhome-rescue)
      (uri /home/user/workspace/NoPCShare/IotTeam/VinhomeDoor/Sources/Hardware/vinhome/vinhome-rescue.lib)))
  (nets
    (net (code 1) (name /Sheet5B6C3003/SCK)
      (node (ref U3) (pin 17))
      (node (ref J11) (pin 7)))
    (net (code 2) (name /Sheet5B6C3003/PD6)
      (node (ref J8) (pin 4))
      (node (ref U3) (pin 10)))
    (net (code 3) (name /Sheet5B6C3003/PD7)
      (node (ref U3) (pin 11))
      (node (ref J8) (pin 5)))
    (net (code 4) (name /Sheet5B616227/BLK)
      (node (ref R9) (pin 1))
      (node (ref U2) (pin 14)))
    (net (code 5) (name /Sheet5B616227/CS_LCD)
      (node (ref R3) (pin 1))
      (node (ref Q4) (pin 3))
      (node (ref U2) (pin 12))
      (node (ref J1) (pin 7)))
    (net (code 6) (name /Sheet5B616227/CS_SD)
      (node (ref U2) (pin 10))
      (node (ref R7) (pin 1))
      (node (ref J7) (pin 4)))
    (net (code 7) (name /Sheet5B616227/CLK)
      (node (ref U2) (pin 22))
      (node (ref J7) (pin 1))
      (node (ref J1) (pin 6)))
    (net (code 8) (name /Sheet5B616227/MOSI)
      (node (ref J1) (pin 5))
      (node (ref J7) (pin 3))
      (node (ref U2) (pin 21)))
    (net (code 9) (name /Sheet5B616227/DC)
      (node (ref J1) (pin 3))
      (node (ref U2) (pin 19)))
    (net (code 10) (name /Sheet5B6C14E0/GPIO10)
      (node (ref U2) (pin 20))
      (node (ref J1) (pin 4)))
    (net (code 11) (name /Sheet5B616227/MISO)
      (node (ref J7) (pin 2))
      (node (ref J1) (pin 1))
      (node (ref U2) (pin 18)))
    (net (code 12) (name /Sheet5B6C3003/PB2)
      (node (ref U3) (pin 14))
      (node (ref J11) (pin 8)))
    (net (code 13) (name /Sheet5B6C3003/PD5)
      (node (ref U3) (pin 9))
      (node (ref J8) (pin 3)))
    (net (code 14) (name /Sheet5B6C3003/MOSI)
      (node (ref J11) (pin 6))
      (node (ref U3) (pin 15)))
    (net (code 15) (name /Sheet5B6C3003/MISO)
      (node (ref U3) (pin 16))
      (node (ref J11) (pin 5)))
    (net (code 16) (name /Sheet5B71ECCF/IRQ)
      (node (ref U3) (pin 32))
      (node (ref J11) (pin 4)))
    (net (code 17) (name /Sheet5B6C3003/PD4)
      (node (ref U3) (pin 2))
      (node (ref J11) (pin 2)))
    (net (code 18) (name /Sheet5B6C3003/PB0)
      (node (ref U3) (pin 12))
      (node (ref J8) (pin 6)))
    (net (code 19) (name /Sheet5B6C14E0/GPIO4)
      (node (ref U2) (pin 13))
      (node (ref U4) (pin 3))
      (node (ref U4) (pin 5)))
    (net (code 20) (name /Sheet5B6162EB/IO0)
      (node (ref J3) (pin 6))
      (node (ref U3) (pin 13)))
    (net (code 21) (name /Sheet5B6162EB/NO)
      (node (ref J3) (pin 4))
      (node (ref U3) (pin 23)))
    (net (code 22) (name /Sheet5B6C3003/PC3)
      (node (ref J3) (pin 3))
      (node (ref U3) (pin 26)))
    (net (code 23) (name /Sheet5B6C3003/PC2)
      (node (ref R1) (pin 2))
      (node (ref U3) (pin 25)))
    (net (code 24) (name /Sheet5B6C14E0/GPIO13)
      (node (ref U2) (pin 7))
      (node (ref J4) (pin 3)))
    (net (code 25) (name /Sheet5B6C14E0/GPIO12)
      (node (ref U2) (pin 6))
      (node (ref J4) (pin 4)))
    (net (code 26) (name /ADC/ADC)
      (node (ref C17) (pin 2))
      (node (ref U2) (pin 2)))
    (net (code 27) (name /Sheet5B6C14E0/GPIO16)
      (node (ref U2) (pin 4))
      (node (ref U3) (pin 1)))
    (net (code 28) (name /Sheet5B6C3003/SCL)
      (node (ref R14) (pin 1))
      (node (ref U2) (pin 5))
      (node (ref U3) (pin 28)))
    (net (code 29) (name /Sheet5B6C3003/SDA)
      (node (ref U2) (pin 11))
      (node (ref R13) (pin 1))
      (node (ref R4) (pin 1))
      (node (ref U3) (pin 27)))
    (net (code 30) (name /Sheet5B6C3003/PC1)
      (node (ref U3) (pin 24))
      (node (ref R12) (pin 2)))
    (net (code 31) (name GND)
      (node (ref C14) (pin 1))
      (node (ref U2) (pin 9))
      (node (ref C8) (pin 2))
      (node (ref C7) (pin 2))
      (node (ref J11) (pin 3))
      (node (ref R19) (pin 2))
      (node (ref C11) (pin 1))
      (node (ref C10) (pin 2))
      (node (ref C13) (pin 1))
      (node (ref J8) (pin 2))
      (node (ref MK1) (pin 1))
      (node (ref C12) (pin 1))
      (node (ref J6) (pin 6))
      (node (ref J6) (pin 2))
      (node (ref R7) (pin 2))
      (node (ref C6) (pin 1))
      (node (ref Y1) (pin 2))
      (node (ref Y1) (pin 4))
      (node (ref U3) (pin 21))
      (node (ref U3) (pin 5))
      (node (ref U3) (pin 3))
      (node (ref C1) (pin 2))
      (node (ref C15) (pin 1))
      (node (ref C3) (pin 2))
      (node (ref U4) (pin 4))
      (node (ref J1) (pin 9))
      (node (ref U4) (pin 1))
      (node (ref Q1) (pin 2))
      (node (ref U1) (pin 4))
      (node (ref U1) (pin 3))
      (node (ref J4) (pin 5))
      (node (ref C2) (pin 2))
      (node (ref C4) (pin 2))
      (node (ref D1) (pin 2))
      (node (ref J2) (pin 1))
      (node (ref C16) (pin 1))
      (node (ref J7) (pin 6))
      (node (ref J5) (pin 2))
      (node (ref R2) (pin 1)))
    (net (code 32) (name +3V3)
      (node (ref J4) (pin 2))
      (node (ref J6) (pin 1))
      (node (ref U1) (pin 2))
      (node (ref U3) (pin 18))
      (node (ref R8) (pin 2))
      (node (ref J6) (pin 8))
      (node (ref U3) (pin 20))
      (node (ref U3) (pin 6))
      (node (ref J3) (pin 5))
      (node (ref C4) (pin 1))
      (node (ref U4) (pin 2))
      (node (ref U3) (pin 4))
      (node (ref C3) (pin 1))
      (node (ref C10) (pin 1))
      (node (ref C8) (pin 1))
      (node (ref Q2) (pin 2))
      (node (ref C14) (pin 2))
      (node (ref J11) (pin 1))
      (node (ref J1) (pin 8))
      (node (ref J5) (pin 1))
      (node (ref U2) (pin 8))
      (node (ref R18) (pin 1))
      (node (ref C16) (pin 2))
      (node (ref J7) (pin 5))
      (node (ref R3) (pin 2))
      (node (ref R4) (pin 2))
      (node (ref R15) (pin 1))
      (node (ref R6) (pin 2))
      (node (ref R13) (pin 2))
      (node (ref R5) (pin 2))
      (node (ref C15) (pin 2))
      (node (ref R14) (pin 2))
      (node (ref C13) (pin 2))
      (node (ref C6) (pin 2))
      (node (ref J8) (pin 1)))
    (net (code 33) (name "Net-(Q2-Pad1)")
      (node (ref Q2) (pin 1))
      (node (ref R9) (pin 2)))
    (net (code 34) (name "Net-(J1-Pad2)")
      (node (ref Q2) (pin 3))
      (node (ref J1) (pin 2)))
    (net (code 35) (name +12V)
      (node (ref U1) (pin 1))
      (node (ref J3) (pin 1))
      (node (ref C1) (pin 1))
      (node (ref J2) (pin 2))
      (node (ref C2) (pin 1)))
    (net (code 36) (name /Sheet5B6162EB/lock)
      (node (ref D1) (pin 1))
      (node (ref Q1) (pin 3))
      (node (ref J3) (pin 2)))
    (net (code 37) (name "Net-(Q1-Pad1)")
      (node (ref R1) (pin 1))
      (node (ref Q1) (pin 1))
      (node (ref R2) (pin 2)))
    (net (code 38) (name "Net-(J4-Pad1)")
      (node (ref J4) (pin 1)))
    (net (code 39) (name "Net-(J10-Pad2)")
      (node (ref U4) (pin 6))
      (node (ref J10) (pin 2)))
    (net (code 40) (name "Net-(J10-Pad1)")
      (node (ref J10) (pin 1))
      (node (ref U4) (pin 7)))
    (net (code 41) (name "Net-(J9-Pad2)")
      (node (ref J9) (pin 2))
      (node (ref U4) (pin 8)))
    (net (code 42) (name "Net-(J9-Pad1)")
      (node (ref U4) (pin 9))
      (node (ref J9) (pin 1)))
    (net (code 43) (name "Net-(Q3-Pad2)")
      (node (ref R10) (pin 1))
      (node (ref Q3) (pin 2)))
    (net (code 44) (name "Net-(Q4-Pad2)")
      (node (ref Q4) (pin 2))
      (node (ref R11) (pin 1)))
    (net (code 45) (name /Sheet5B6C14E0/RST_ESP)
      (node (ref C7) (pin 1))
      (node (ref R12) (pin 1))
      (node (ref R6) (pin 1))
      (node (ref U2) (pin 1))
      (node (ref Q3) (pin 3)))
    (net (code 46) (name /Sheet5B6C14E0/DTR)
      (node (ref Q4) (pin 1))
      (node (ref R10) (pin 2))
      (node (ref J5) (pin 6)))
    (net (code 47) (name /Sheet5B6C14E0/RTS)
      (node (ref J5) (pin 5))
      (node (ref R11) (pin 2))
      (node (ref Q3) (pin 1)))
    (net (code 48) (name "Net-(U2-Pad17)")
      (node (ref U2) (pin 17)))
    (net (code 49) (name /Sheet5B6C14E0/TXD)
      (node (ref J5) (pin 3))
      (node (ref U2) (pin 16)))
    (net (code 50) (name /Sheet5B6C14E0/RXD)
      (node (ref J5) (pin 4))
      (node (ref U2) (pin 15)))
    (net (code 51) (name /Sheet5B6C14E0/CH_PD)
      (node (ref R5) (pin 1))
      (node (ref U2) (pin 3)))
    (net (code 52) (name "Net-(C11-Pad2)")
      (node (ref U3) (pin 7))
      (node (ref Y1) (pin 1))
      (node (ref C11) (pin 2)))
    (net (code 53) (name "Net-(C12-Pad2)")
      (node (ref C12) (pin 2))
      (node (ref U3) (pin 8))
      (node (ref Y1) (pin 3)))
    (net (code 54) (name "Net-(U3-Pad22)")
      (node (ref U3) (pin 22)))
    (net (code 55) (name /Sheet5B6C3003/RESET)
      (node (ref C9) (pin 1))
      (node (ref J6) (pin 7))
      (node (ref U3) (pin 29))
      (node (ref R8) (pin 1)))
    (net (code 56) (name "Net-(U3-Pad19)")
      (node (ref U3) (pin 19)))
    (net (code 57) (name "Net-(C9-Pad2)")
      (node (ref J6) (pin 5))
      (node (ref C9) (pin 2)))
    (net (code 58) (name /Sheet5B6C3003/RXD_AT)
      (node (ref J6) (pin 4))
      (node (ref U3) (pin 30)))
    (net (code 59) (name /Sheet5B6C3003/TXD_AT)
      (node (ref J6) (pin 3))
      (node (ref U3) (pin 31)))
    (net (code 60) (name "Net-(C5-Pad2)")
      (node (ref R16) (pin 2))
      (node (ref Q5) (pin 1))
      (node (ref C5) (pin 2)))
    (net (code 61) (name "Net-(C5-Pad1)")
      (node (ref C5) (pin 1))
      (node (ref R15) (pin 2))
      (node (ref MK1) (pin 2)))
    (net (code 62) (name "Net-(C17-Pad1)")
      (node (ref Q5) (pin 3))
      (node (ref R16) (pin 1))
      (node (ref R18) (pin 2))
      (node (ref C17) (pin 1)))
    (net (code 63) (name "Net-(Q5-Pad2)")
      (node (ref Q5) (pin 2))
      (node (ref R19) (pin 1)))))