(export (version D)
  (design
    (source /home/user/workspace/NoPCShare/IotTeam/VinhomeDoor/Sources/Hardware/vinhome/keypad/keypad.sch)
    (date "Thu 27 Sep 2018 05:10:15 PM +07")
    (tool "Eeschema (5.0.0-rc2-109-g0e3be5776-dirty)-sonnt")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source keypad.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref U9)
      (value ttp229)
      (footprint Housings_SSOP:SSOP-28_3.9x9.9mm_Pitch0.635mm)
      (libsource (lib keypad-rescue) (part ttp229-lanhnd) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B8F5AD2))
    (comp (ref U22)
      (value ttp229)
      (footprint Housings_SSOP:SSOP-28_3.9x9.9mm_Pitch0.635mm)
      (libsource (lib keypad-rescue) (part ttp229-lanhnd) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B8F5C74))
    (comp (ref C16)
      (value 106)
      (footprint Capacitors_SMD:C_0805_HandSoldering)
      (libsource (lib device) (part C_Small) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B8F657D))
    (comp (ref C15)
      (value 104)
      (footprint Capacitors_SMD:C_0805_HandSoldering)
      (libsource (lib device) (part C_Small) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B8F665D))
    (comp (ref U1)
      (value touch)
      (footprint iot:touch)
      (libsource (lib keypad-rescue) (part touch-lanhnd) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B8FA2EE))
    (comp (ref U2)
      (value touch)
      (footprint iot:touch)
      (libsource (lib keypad-rescue) (part touch-lanhnd) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B8FA477))
    (comp (ref U3)
      (value touch)
      (footprint iot:touch)
      (libsource (lib keypad-rescue) (part touch-lanhnd) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B8FA501))
    (comp (ref U4)
      (value touch)
      (footprint iot:touch)
      (libsource (lib keypad-rescue) (part touch-lanhnd) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B8FA781))
    (comp (ref U5)
      (value touch)
      (footprint iot:touch)
      (libsource (lib keypad-rescue) (part touch-lanhnd) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B8FA859))
    (comp (ref U6)
      (value touch)
      (footprint iot:touch)
      (libsource (lib keypad-rescue) (part touch-lanhnd) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B8FA889))
    (comp (ref U7)
      (value touch)
      (footprint iot:touch)
      (libsource (lib keypad-rescue) (part touch-lanhnd) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B8FA8B7))
    (comp (ref U8)
      (value touch)
      (footprint iot:touch)
      (libsource (lib keypad-rescue) (part touch-lanhnd) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B8FA8E7))
    (comp (ref U10)
      (value touch)
      (footprint iot:touch)
      (libsource (lib keypad-rescue) (part touch-lanhnd) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B8FBC64))
    (comp (ref U11)
      (value touch)
      (footprint iot:touch)
      (libsource (lib keypad-rescue) (part touch-lanhnd) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B8FBC6B))
    (comp (ref U12)
      (value touch)
      (footprint iot:touch)
      (libsource (lib keypad-rescue) (part touch-lanhnd) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B8FBC72))
    (comp (ref U13)
      (value touch)
      (footprint iot:touch)
      (libsource (lib keypad-rescue) (part touch-lanhnd) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B8FBC79))
    (comp (ref U14)
      (value touch)
      (footprint iot:touch)
      (libsource (lib keypad-rescue) (part touch-lanhnd) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B8FBC80))
    (comp (ref U15)
      (value touch)
      (footprint iot:touch)
      (libsource (lib keypad-rescue) (part touch-lanhnd) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B8FBC87))
    (comp (ref U16)
      (value touch)
      (footprint iot:touch)
      (libsource (lib keypad-rescue) (part touch-lanhnd) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B8FBC8E))
    (comp (ref U17)
      (value touch)
      (footprint iot:touch)
      (libsource (lib keypad-rescue) (part touch-lanhnd) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B8FBC95))
    (comp (ref U18)
      (value touch)
      (footprint iot:touch)
      (libsource (lib keypad-rescue) (part touch-lanhnd) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B8FD682))
    (comp (ref U19)
      (value touch)
      (footprint iot:touch)
      (libsource (lib keypad-rescue) (part touch-lanhnd) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B8FD689))
    (comp (ref U20)
      (value touch)
      (footprint iot:touch)
      (libsource (lib keypad-rescue) (part touch-lanhnd) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B8FD690))
    (comp (ref U21)
      (value touch)
      (footprint iot:touch)
      (libsource (lib keypad-rescue) (part touch-lanhnd) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B8FD697))
    (comp (ref C1)
      (value 0-50pF)
      (footprint Capacitors_SMD:C_0805_HandSoldering)
      (libsource (lib device) (part C_Variable) (description "Variable capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B900EE6))
    (comp (ref C2)
      (value 0-50pF)
      (footprint Capacitors_SMD:C_0805_HandSoldering)
      (libsource (lib device) (part C_Variable) (description "Variable capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B90123B))
    (comp (ref C3)
      (value 0-50pF)
      (footprint Capacitors_SMD:C_0805_HandSoldering)
      (libsource (lib device) (part C_Variable) (description "Variable capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B9012CB))
    (comp (ref C6)
      (value 0-50pF)
      (footprint Capacitors_SMD:C_0805_HandSoldering)
      (libsource (lib device) (part C_Variable) (description "Variable capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B901386))
    (comp (ref C5)
      (value 0-50pF)
      (footprint Capacitors_SMD:C_0805_HandSoldering)
      (libsource (lib device) (part C_Variable) (description "Variable capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B901406))
    (comp (ref C4)
      (value 0-50pF)
      (footprint Capacitors_SMD:C_0805_HandSoldering)
      (libsource (lib device) (part C_Variable) (description "Variable capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B901535))
    (comp (ref C9)
      (value 0-50pF)
      (footprint Capacitors_SMD:C_0805_HandSoldering)
      (libsource (lib device) (part C_Variable) (description "Variable capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B901603))
    (comp (ref C10)
      (value 0-50pF)
      (footprint Capacitors_SMD:C_0805_HandSoldering)
      (libsource (lib device) (part C_Variable) (description "Variable capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B901687))
    (comp (ref C11)
      (value 0-50pF)
      (footprint Capacitors_SMD:C_0805_HandSoldering)
      (libsource (lib device) (part C_Variable) (description "Variable capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B9016F1))
    (comp (ref C13)
      (value 0-50pF)
      (footprint Capacitors_SMD:C_0805_HandSoldering)
      (libsource (lib device) (part C_Variable) (description "Variable capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B901757))
    (comp (ref C12)
      (value 0-50pF)
      (footprint Capacitors_SMD:C_0805_HandSoldering)
      (libsource (lib device) (part C_Variable) (description "Variable capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B9017D3))
    (comp (ref C14)
      (value 0-50pF)
      (footprint Capacitors_SMD:C_0805_HandSoldering)
      (libsource (lib device) (part C_Variable) (description "Variable capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B901845))
    (comp (ref C7)
      (value 104)
      (footprint Capacitors_SMD:C_0805_HandSoldering)
      (libsource (lib device) (part C_Small) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B93E69D))
    (comp (ref C8)
      (value 106)
      (footprint Capacitors_SMD:C_0805_HandSoldering)
      (libsource (lib device) (part C_Small) (description "Unpolarized capacitor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B93E92D))
    (comp (ref J1)
      (value Conn_01x06)
      (footprint Pin_Headers:Pin_Header_Straight_1x06_Pitch2.54mm)
      (datasheet ~)
      (libsource (lib Connector) (part Conn_01x06) (description "Generic connector, single row, 01x06"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B9D1E41))
    (comp (ref R2)
      (value 820K)
      (footprint Resistors_SMD:R_0805)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B927AF0))
    (comp (ref R3)
      (value 820K)
      (footprint Resistors_SMD:R_0805)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5B927B54))
    (comp (ref R1)
      (value 820K)
      (footprint Resistors_SMD:R_0805)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BADE8D8))
    (comp (ref R4)
      (value 820K)
      (footprint Resistors_SMD:R_0805)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BADEA6C))
    (comp (ref R8)
      (value 820K)
      (footprint Resistors_SMD:R_0805)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BB04221))
    (comp (ref R7)
      (value 820K)
      (footprint Resistors_SMD:R_0805)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BB042C3))
    (comp (ref R6)
      (value 820K)
      (footprint Resistors_SMD:R_0805)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BB04341))
    (comp (ref R5)
      (value 820K)
      (footprint Resistors_SMD:R_0805)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BB043BB))
    (comp (ref R12)
      (value 820K)
      (footprint Resistors_SMD:R_0805)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BB38E9D))
    (comp (ref R11)
      (value 820K)
      (footprint Resistors_SMD:R_0805)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BB38FAF))
    (comp (ref R10)
      (value 820K)
      (footprint Resistors_SMD:R_0805)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BB39135))
    (comp (ref R9)
      (value 820K)
      (footprint Resistors_SMD:R_0805)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BB391CD))
    (comp (ref R16)
      (value 820K)
      (footprint Resistors_SMD:R_0805)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BB39361))
    (comp (ref R15)
      (value 820K)
      (footprint Resistors_SMD:R_0805)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BB393F9))
    (comp (ref R14)
      (value 820K)
      (footprint Resistors_SMD:R_0805)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BB39483))
    (comp (ref R13)
      (value 820K)
      (footprint Resistors_SMD:R_0805)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BB39513))
    (comp (ref R20)
      (value 820K)
      (footprint Resistors_SMD:R_0805)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BB44F7E))
    (comp (ref R19)
      (value 820K)
      (footprint Resistors_SMD:R_0805)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BB45018))
    (comp (ref R18)
      (value 820K)
      (footprint Resistors_SMD:R_0805)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BB450A4))
    (comp (ref R17)
      (value 820K)
      (footprint Resistors_SMD:R_0805)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BB4512E))
    (comp (ref R21)
      (value 820K)
      (footprint Resistors_SMD:R_0805)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BC25C35))
    (comp (ref R22)
      (value 0R)
      (footprint Resistors_SMD:R_0805)
      (libsource (lib device) (part R) (description Resistor))
      (sheetpath (names /) (tstamps /))
      (tstamp 5BAD55B2)))
  (libparts
    (libpart (lib Connector) (part Conn_01x06)
      (description "Generic connector, single row, 01x06")
      (docs ~)
      (footprints
        (fp Connector*:*_??x*mm*)
        (fp Connector*:*1x??x*mm*)
        (fp Pin?Header?Straight?1X*)
        (fp Pin?Header?Angled?1X*)
        (fp Socket?Strip?Straight?1X*)
        (fp Socket?Strip?Angled?1X*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x06))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))
        (pin (num 4) (name Pin_4) (type passive))
        (pin (num 5) (name Pin_5) (type passive))
        (pin (num 6) (name Pin_6) (type passive))))
    (libpart (lib device) (part C_Small)
      (description "Unpolarized capacitor")
      (footprints
        (fp C_*))
      (fields
        (field (name Reference) C)
        (field (name Value) C_Small))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib device) (part C_Variable)
      (description "Variable capacitor")
      (fields
        (field (name Reference) C)
        (field (name Value) C_Variable))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib device) (part R)
      (description Resistor)
      (footprints
        (fp R_*)
        (fp R_*))
      (fields
        (field (name Reference) R)
        (field (name Value) R))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib keypad-rescue) (part touch-lanhnd)
      (fields
        (field (name Reference) U)
        (field (name Value) touch-lanhnd))
      (pins
        (pin (num 1) (name _) (type input))))
    (libpart (lib keypad-rescue) (part ttp229-lanhnd)
      (fields
        (field (name Reference) U)
        (field (name Value) ttp229-lanhnd))
      (pins
        (pin (num 1) (name TP3) (type input))
        (pin (num 2) (name TP2) (type input))
        (pin (num 3) (name NC) (type input))
        (pin (num 4) (name SENADJ0) (type input))
        (pin (num 5) (name TP1) (type input))
        (pin (num 6) (name TP0) (type input))
        (pin (num 7) (name TP15) (type input))
        (pin (num 8) (name TP14) (type input))
        (pin (num 9) (name SENADJ3) (type input))
        (pin (num 10) (name TP13) (type input))
        (pin (num 11) (name TP12) (type input))
        (pin (num 12) (name SD0) (type input))
        (pin (num 13) (name SCL) (type input))
        (pin (num 14) (name SLPSENB) (type input))
        (pin (num 15) (name TP11) (type input))
        (pin (num 16) (name TP10) (type input))
        (pin (num 17) (name SENADJ2) (type input))
        (pin (num 18) (name TP9) (type input))
        (pin (num 19) (name TP8) (type input))
        (pin (num 20) (name TEST) (type input))
        (pin (num 21) (name TP7) (type input))
        (pin (num 22) (name TP6) (type input))
        (pin (num 23) (name SENADJ1) (type input))
        (pin (num 24) (name TP5) (type input))
        (pin (num 25) (name TP4) (type input))
        (pin (num 26) (name VDD) (type input))
        (pin (num 27) (name VSS) (type input))
        (pin (num 28) (name SLPSENA) (type input)))))
  (libraries
    (library (logical Connector)
      (uri /usr/share/kicad/library//Connector.lib))
    (library (logical device)
      (uri /usr/share/kicad/library//device.lib))
    (library (logical keypad-rescue)
      (uri /home/user/workspace/NoPCShare/IotTeam/VinhomeDoor/Sources/Hardware/vinhome/keypad/keypad-rescue.lib)))
  (nets
    (net (code 1) (name /SCL2)
      (node (ref U22) (pin 13))
      (node (ref J1) (pin 6)))
    (net (code 2) (name /K21)
      (node (ref R21) (pin 1))
      (node (ref U22) (pin 25)))
    (net (code 3) (name /K4)
      (node (ref U4) (pin 1))
      (node (ref R2) (pin 1))
      (node (ref U9) (pin 1)))
    (net (code 4) (name /K3)
      (node (ref U3) (pin 1))
      (node (ref U9) (pin 2))
      (node (ref R3) (pin 1)))
    (net (code 5) (name /SDO2)
      (node (ref U22) (pin 12))
      (node (ref R22) (pin 2))
      (node (ref J1) (pin 5)))
    (net (code 6) (name /SCL1)
      (node (ref J1) (pin 4))
      (node (ref U9) (pin 13)))
    (net (code 7) (name /SDO1)
      (node (ref J1) (pin 3))
      (node (ref U9) (pin 12))
      (node (ref R22) (pin 1)))
    (net (code 8) (name +5V)
      (node (ref C7) (pin 2))
      (node (ref C8) (pin 2))
      (node (ref U22) (pin 26))
      (node (ref C15) (pin 2))
      (node (ref U9) (pin 26))
      (node (ref C16) (pin 2))
      (node (ref J1) (pin 2)))
    (net (code 9) (name /K20)
      (node (ref R17) (pin 1))
      (node (ref U22) (pin 1))
      (node (ref U21) (pin 1)))
    (net (code 10) (name GND)
      (node (ref C5) (pin 1))
      (node (ref R12) (pin 2))
      (node (ref C15) (pin 1))
      (node (ref C16) (pin 1))
      (node (ref C4) (pin 1))
      (node (ref R11) (pin 2))
      (node (ref R17) (pin 2))
      (node (ref R18) (pin 2))
      (node (ref C14) (pin 1))
      (node (ref C12) (pin 1))
      (node (ref C13) (pin 1))
      (node (ref C11) (pin 2))
      (node (ref C10) (pin 2))
      (node (ref C3) (pin 2))
      (node (ref C2) (pin 2))
      (node (ref C1) (pin 2))
      (node (ref U9) (pin 27))
      (node (ref U9) (pin 20))
      (node (ref U22) (pin 27))
      (node (ref C9) (pin 2))
      (node (ref U22) (pin 20))
      (node (ref C8) (pin 1))
      (node (ref C7) (pin 1))
      (node (ref C6) (pin 1))
      (node (ref R8) (pin 2))
      (node (ref R7) (pin 2))
      (node (ref R6) (pin 2))
      (node (ref R5) (pin 2))
      (node (ref R9) (pin 2))
      (node (ref R1) (pin 2))
      (node (ref R4) (pin 2))
      (node (ref R3) (pin 2))
      (node (ref R2) (pin 2))
      (node (ref J1) (pin 1))
      (node (ref R10) (pin 2))
      (node (ref R19) (pin 2))
      (node (ref R20) (pin 2))
      (node (ref R21) (pin 2))
      (node (ref R13) (pin 2))
      (node (ref R14) (pin 2))
      (node (ref R16) (pin 2))
      (node (ref R15) (pin 2)))
    (net (code 11) (name /K19)
      (node (ref R18) (pin 1))
      (node (ref U22) (pin 2))
      (node (ref U20) (pin 1)))
    (net (code 12) (name /K18)
      (node (ref U19) (pin 1))
      (node (ref U22) (pin 5))
      (node (ref R19) (pin 1)))
    (net (code 13) (name /K17)
      (node (ref U22) (pin 6))
      (node (ref R20) (pin 1))
      (node (ref U18) (pin 1)))
    (net (code 14) (name "Net-(U22-Pad3)")
      (node (ref U22) (pin 3)))
    (net (code 15) (name /K8)
      (node (ref R5) (pin 1))
      (node (ref U8) (pin 1))
      (node (ref U9) (pin 21)))
    (net (code 16) (name /K7)
      (node (ref U7) (pin 1))
      (node (ref U9) (pin 22))
      (node (ref R6) (pin 1)))
    (net (code 17) (name /K6)
      (node (ref U9) (pin 24))
      (node (ref U6) (pin 1))
      (node (ref R7) (pin 1)))
    (net (code 18) (name /K5)
      (node (ref U9) (pin 25))
      (node (ref U5) (pin 1))
      (node (ref R8) (pin 1)))
    (net (code 19) (name /K2)
      (node (ref U9) (pin 5))
      (node (ref U2) (pin 1))
      (node (ref R1) (pin 1)))
    (net (code 20) (name /K1)
      (node (ref U9) (pin 6))
      (node (ref U1) (pin 1))
      (node (ref R4) (pin 1)))
    (net (code 21) (name "Net-(U22-Pad8)")
      (node (ref U22) (pin 8)))
    (net (code 22) (name "Net-(U22-Pad24)")
      (node (ref U22) (pin 24)))
    (net (code 23) (name "Net-(U22-Pad22)")
      (node (ref U22) (pin 22)))
    (net (code 24) (name "Net-(U22-Pad21)")
      (node (ref U22) (pin 21)))
    (net (code 25) (name "Net-(U22-Pad19)")
      (node (ref U22) (pin 19)))
    (net (code 26) (name "Net-(U22-Pad18)")
      (node (ref U22) (pin 18)))
    (net (code 27) (name "Net-(U22-Pad15)")
      (node (ref U22) (pin 15)))
    (net (code 28) (name "Net-(U22-Pad16)")
      (node (ref U22) (pin 16)))
    (net (code 29) (name "Net-(U22-Pad11)")
      (node (ref U22) (pin 11)))
    (net (code 30) (name "Net-(U22-Pad10)")
      (node (ref U22) (pin 10)))
    (net (code 31) (name "Net-(U22-Pad7)")
      (node (ref U22) (pin 7)))
    (net (code 32) (name "Net-(C14-Pad2)")
      (node (ref C14) (pin 2))
      (node (ref U22) (pin 28)))
    (net (code 33) (name /K16)
      (node (ref R13) (pin 1))
      (node (ref U17) (pin 1))
      (node (ref U9) (pin 7)))
    (net (code 34) (name /K15)
      (node (ref U16) (pin 1))
      (node (ref R14) (pin 1))
      (node (ref U9) (pin 8)))
    (net (code 35) (name /K14)
      (node (ref U15) (pin 1))
      (node (ref U9) (pin 10))
      (node (ref R15) (pin 1)))
    (net (code 36) (name /K13)
      (node (ref U14) (pin 1))
      (node (ref U9) (pin 11))
      (node (ref R16) (pin 1)))
    (net (code 37) (name /K12)
      (node (ref U9) (pin 15))
      (node (ref U13) (pin 1))
      (node (ref R9) (pin 1)))
    (net (code 38) (name /K11)
      (node (ref U12) (pin 1))
      (node (ref U9) (pin 16))
      (node (ref R10) (pin 1)))
    (net (code 39) (name /K10)
      (node (ref U11) (pin 1))
      (node (ref R11) (pin 1))
      (node (ref U9) (pin 18)))
    (net (code 40) (name /K9)
      (node (ref R12) (pin 1))
      (node (ref U9) (pin 19))
      (node (ref U10) (pin 1)))
    (net (code 41) (name "Net-(U9-Pad3)")
      (node (ref U9) (pin 3)))
    (net (code 42) (name "Net-(C5-Pad2)")
      (node (ref C5) (pin 2))
      (node (ref U9) (pin 23)))
    (net (code 43) (name "Net-(C2-Pad1)")
      (node (ref C2) (pin 1))
      (node (ref U9) (pin 9)))
    (net (code 44) (name "Net-(C1-Pad1)")
      (node (ref C1) (pin 1))
      (node (ref U9) (pin 4)))
    (net (code 45) (name "Net-(C4-Pad2)")
      (node (ref C4) (pin 2))
      (node (ref U9) (pin 28)))
    (net (code 46) (name "Net-(C6-Pad2)")
      (node (ref U9) (pin 17))
      (node (ref C6) (pin 2)))
    (net (code 47) (name "Net-(C3-Pad1)")
      (node (ref U9) (pin 14))
      (node (ref C3) (pin 1)))
    (net (code 48) (name "Net-(C10-Pad1)")
      (node (ref C10) (pin 1))
      (node (ref U22) (pin 9)))
    (net (code 49) (name "Net-(C9-Pad1)")
      (node (ref C9) (pin 1))
      (node (ref U22) (pin 4)))
    (net (code 50) (name "Net-(C12-Pad2)")
      (node (ref U22) (pin 23))
      (node (ref C12) (pin 2)))
    (net (code 51) (name "Net-(C13-Pad2)")
      (node (ref C13) (pin 2))
      (node (ref U22) (pin 17)))
    (net (code 52) (name "Net-(C11-Pad1)")
      (node (ref C11) (pin 1))
      (node (ref U22) (pin 14)))))